Command: ninja flash
[1/5] cd /mnt/douwe/hdd/Projects/SerreklimaatSensor/build && /home/douwe/.espressif/tools/python/v6.0/venv/bin/python /home/douwe/.espressif/v6.0/esp-idf/components/partition_table/check_sizes.py --offset 0x8000 partition --type app /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/partition_table/partition-table.bin /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/dht11_reader.bin
dht11_reader.bin binary size 0x32110 bytes. Smallest app partition is 0x1e0000 bytes. 0x1adef0 bytes (90%) free.
[2/5] Performing build step for 'bootloader'
[1/1] cd /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/bootloader && /home/douwe/.espressif/tools/python/v6.0/venv/bin/python /home/douwe/.espressif/v6.0/esp-idf/components/partition_table/check_sizes.py --offset 0x8000 bootloader 0x0 /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/bootloader/bootloader.bin
Bootloader binary size 0x5250 bytes. 0x2db0 bytes (36%) free.
[3/5] No install step for 'bootloader'
[4/5] Completed 'bootloader'
[4/5] Running utility command for flash
esptool --chip esp32c3 -p /dev/ttyACM0 -b 460800 --before=default-reset --after=hard-reset write-flash --flash-mode dio --flash-freq 80m --flash-size 2MB 0x0 bootloader/bootloader.bin 0x8000 partition_table/partition-table.bin 0x10000 dht11_reader.bin
esptool v5.3.dev2
Serial port /dev/ttyACM0:
Connecting...
[1A[2K[1A[2KConnected to ESP32-C3 on /dev/ttyACM0:
Chip type:          ESP32-C3 (QFN32) (revision v0.4)
Features:           Wi-Fi, BT 5 (LE), Single Core, 160MHz, Embedded Flash 4MB (XMC)
Crystal frequency:  40MHz
USB mode:           USB-Serial/JTAG
MAC:                ac:a7:04:d0:82:b4

Uploading stub flasher...
Running stub flasher...
[1A[2K[1A[2KStub flasher running.
Changing baud rate to 460800...
Changed.

Configuring flash size...

Writing 'bootloader/bootloader.bin' at 0x00000000...
SHA digest in image updated.
Flash will be erased from 0x00000000 to 0x00005fff...
Compressed 21072 bytes to 13351...

[KWriting at 0x00000000 [                              ]   0.0% 0/13351 bytes... 
[KWriting at 0x00005250 [==============================] 100.0% 13351/13351 bytes... 
[1A[2K[1A[2KWrote 21072 bytes (13351 compressed) at 0x00000000 in 0.3 seconds (637.7 kbit/s).
Verifying written data...
[1A[2KHash of data verified.

Writing 'partition_table/partition-table.bin' at 0x00008000...
Flash will be erased from 0x00008000 to 0x00008fff...
Compressed 3072 bytes to 118...

[KWriting at 0x00008000 [                              ]   0.0% 0/118 bytes... 
[KWriting at 0x00008c00 [==============================] 100.0% 118/118 bytes... 
[1A[2K[1A[2KWrote 3072 bytes (118 compressed) at 0x00008000 in 0.0 seconds (793.1 kbit/s).
Verifying written data...
[1A[2KHash of data verified.

Writing 'dht11_reader.bin' at 0x00010000...
Flash will be erased from 0x00010000 to 0x00042fff...
Compressed 205072 bytes to 114141...

[KWriting at 0x00010000 [                              ]   0.0% 0/114141 bytes... 
[KWriting at 0x0001a505 [===>                          ]  14.4% 16384/114141 bytes... 
[KWriting at 0x00020c3b [=======>                      ]  28.7% 32768/114141 bytes... 
[KWriting at 0x0002797d [===========>                  ]  43.1% 49152/114141 bytes... 
[KWriting at 0x0002eaf6 [================>             ]  57.4% 65536/114141 bytes... 
[KWriting at 0x000353b8 [====================>         ]  71.8% 81920/114141 bytes... 
[KWriting at 0x0003ae2e [========================>     ]  86.1% 98304/114141 bytes... 
[KWriting at 0x00042110 [==============================] 100.0% 114141/114141 bytes... 
[1A[2K[1A[2KWrote 205072 bytes (114141 compressed) at 0x00010000 in 1.2 seconds (1391.0 kbit/s).
Verifying written data...
[1A[2KHash of data verified.

Hard resetting via RTS pin...
