Command: ninja flash
[1/5] cd /home/douwe/Projects/temperature_measure/build && /home/douwe/.espressif/tools/python/v6.0/venv/bin/python /home/douwe/.espressif/v6.0/esp-idf/components/partition_table/check_sizes.py --offset 0x8000 partition --type app /home/douwe/Projects/temperature_measure/build/partition_table/partition-table.bin /home/douwe/Projects/temperature_measure/build/dht11_reader.bin
dht11_reader.bin binary size 0x212b0 bytes. Smallest app partition is 0x100000 bytes. 0xded50 bytes (87%) free.
[2/5] Performing build step for 'bootloader'
[1/1] cd /home/douwe/Projects/temperature_measure/build/bootloader && /home/douwe/.espressif/tools/python/v6.0/venv/bin/python /home/douwe/.espressif/v6.0/esp-idf/components/partition_table/check_sizes.py --offset 0x8000 bootloader 0x0 /home/douwe/Projects/temperature_measure/build/bootloader/bootloader.bin
Bootloader binary size 0x5250 bytes. 0x2db0 bytes (36%) free.
[3/5] No install step for 'bootloader'
[4/5] Completed 'bootloader'
[4/5] Running utility command for flash
esptool --chip esp32c3 -p /dev/ttyACM0 -b 460800 --before=default-reset --after=hard-reset write-flash --flash-mode dio --flash-freq 80m --flash-size 2MB 0x0 bootloader/bootloader.bin 0x8000 partition_table/partition-table.bin 0x10000 dht11_reader.bin
esptool v5.3.dev2
Serial port /dev/ttyACM0:
Connecting...
[1A[2K[1A[2KConnected to ESP32-C3 on /dev/ttyACM0:
Chip type:          ESP32-C3 (QFN32) (revision v0.4)
Features:           Wi-Fi, BT 5 (LE), Single Core, 160MHz, Embedded Flash 4MB (XMC)
Crystal frequency:  40MHz
USB mode:           USB-Serial/JTAG
MAC:                ac:a7:04:d0:82:b4

Uploading stub flasher...
Running stub flasher...
[1A[2K[1A[2KStub flasher running.
Changing baud rate to 460800...
Changed.

Configuring flash size...

Writing 'bootloader/bootloader.bin' at 0x00000000...
SHA digest in image updated.
Flash will be erased from 0x00000000 to 0x00005fff...
Compressed 21072 bytes to 13350...

[KWriting at 0x00000000 [                              ]   0.0% 0/13350 bytes... 
[KWriting at 0x00005250 [==============================] 100.0% 13350/13350 bytes... 
[1A[2K[1A[2KWrote 21072 bytes (13350 compressed) at 0x00000000 in 0.2 seconds (901.8 kbit/s).
Verifying written data...
[1A[2KHash of data verified.

Writing 'partition_table/partition-table.bin' at 0x00008000...
Flash will be erased from 0x00008000 to 0x00008fff...
Compressed 3072 bytes to 103...

[KWriting at 0x00008000 [                              ]   0.0% 0/103 bytes... 
[KWriting at 0x00008c00 [==============================] 100.0% 103/103 bytes... 
[1A[2K[1A[2KWrote 3072 bytes (103 compressed) at 0x00008000 in 0.0 seconds (962.7 kbit/s).
Verifying written data...
[1A[2KHash of data verified.

Writing 'dht11_reader.bin' at 0x00010000...
Flash will be erased from 0x00010000 to 0x00031fff...
Compressed 135856 bytes to 76775...

[KWriting at 0x00010000 [                              ]   0.0% 0/76775 bytes... 
[KWriting at 0x000191b4 [=====>                        ]  21.3% 16384/76775 bytes... 
[KWriting at 0x0001fc62 [===========>                  ]  42.7% 32768/76775 bytes... 
[KWriting at 0x0002674a [==================>           ]  64.0% 49152/76775 bytes... 
[KWriting at 0x0002c9ff [========================>     ]  85.4% 65536/76775 bytes... 
[KWriting at 0x000312b0 [==============================] 100.0% 76775/76775 bytes... 
[1A[2K[1A[2KWrote 135856 bytes (76775 compressed) at 0x00010000 in 0.6 seconds (1939.8 kbit/s).
Verifying written data...
[1A[2KHash of data verified.

Hard resetting via RTS pin...
