Command: ninja all
[0/1] Re-running CMake...
-- Component directory /home/douwe/.espressif/v6.0/esp-idf/components/mqtt does not contain a CMakeLists.txt file. No component will be added
-- Minimal build - ON
-- Building ESP-IDF components for target esp32c3
-- ESP-TEE is currently supported only on the esp32c6;esp32h2;esp32c5;esp32c61 SoCs
-- KCONFIG_REPORT_VERBOSITY not set, using default
-- Project sdkconfig file /mnt/douwe/hdd/Projects/SerreklimaatSensor/sdkconfig
-- Detecting C compiler ABI info
-- Detecting C compiler ABI info - done
-- Detecting CXX compiler ABI info
-- Detecting CXX compiler ABI info - done
-- Detecting C compiler ABI info
-- Detecting C compiler ABI info - done
-- Detecting CXX compiler ABI info
-- Detecting CXX compiler ABI info - done
-- Detecting C compiler ABI info
-- Detecting C compiler ABI info - done
-- Detecting CXX compiler ABI info
-- Detecting CXX compiler ABI info - done
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/riscv/ld/rom.api.ld
-- App "dht11_reader" version: 1d246d6-dirty
-- Setting up mbedtls configuration
-- Linkage type is PUBLIC
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_system/ld/esp32c3/memory.ld.in
--   -> Preprocessing .in script: /home/douwe/.espressif/v6.0/esp-idf/components/esp_system/ld/esp32c3/memory.ld.in
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_system/ld/esp32c3/sections.ld.in
--   -> Preprocessing .in script: /home/douwe/.espressif/v6.0/esp-idf/components/esp_system/ld/esp32c3/sections.ld.in
--   -> Applying ldgen processing: /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/esp-idf/esp_system/ld/sections.ld.in
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.api.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.bt_funcs.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.libgcc.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.version.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ble_master.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ble_50.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ble_smp.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ble_dtm.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ble_test.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ble_scan.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.eco3.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.eco3_bt_funcs.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.libc.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/soc/esp32c3/ld/esp32c3.peripherals.ld
-- Components: app_update bootloader bootloader_support cxx efuse esp_app_format esp_blockdev esp_bootloader_format esp_common esp_driver_dma esp_driver_gpio esp_driver_uart esp_driver_usb_serial_jtag esp_hal_ana_conv esp_hal_clock esp_hal_dma esp_hal_gpio esp_hal_gpspi esp_hal_i2s esp_hal_mspi esp_hal_pmu esp_hal_rtc_timer esp_hal_security esp_hal_timg esp_hal_touch_sens esp_hal_uart esp_hal_usb esp_hal_wdt esp_hw_support esp_libc esp_mm esp_partition esp_pm esp_psram esp_ringbuf esp_rom esp_security esp_stdio esp_system esp_timer esp_usb_cdc_rom_console esptool_py freertos hal heap log main mbedtls partition_table pthread riscv soc spi_flash spiffs vfs
-- Component paths: /home/douwe/.espressif/v6.0/esp-idf/components/app_update /home/douwe/.espressif/v6.0/esp-idf/components/bootloader /home/douwe/.espressif/v6.0/esp-idf/components/bootloader_support /home/douwe/.espressif/v6.0/esp-idf/components/cxx /home/douwe/.espressif/v6.0/esp-idf/components/efuse /home/douwe/.espressif/v6.0/esp-idf/components/esp_app_format /home/douwe/.espressif/v6.0/esp-idf/components/esp_blockdev /home/douwe/.espressif/v6.0/esp-idf/components/esp_bootloader_format /home/douwe/.espressif/v6.0/esp-idf/components/esp_common /home/douwe/.espressif/v6.0/esp-idf/components/esp_driver_dma /home/douwe/.espressif/v6.0/esp-idf/components/esp_driver_gpio /home/douwe/.espressif/v6.0/esp-idf/components/esp_driver_uart /home/douwe/.espressif/v6.0/esp-idf/components/esp_driver_usb_serial_jtag /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_ana_conv /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_clock /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_dma /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_gpio /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_gpspi /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_i2s /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_mspi /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_pmu /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_rtc_timer /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_security /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_timg /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_touch_sens /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_uart /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_usb /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_wdt /home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support /home/douwe/.espressif/v6.0/esp-idf/components/esp_libc /home/douwe/.espressif/v6.0/esp-idf/components/esp_mm /home/douwe/.espressif/v6.0/esp-idf/components/esp_partition /home/douwe/.espressif/v6.0/esp-idf/components/esp_pm /home/douwe/.espressif/v6.0/esp-idf/components/esp_psram /home/douwe/.espressif/v6.0/esp-idf/components/esp_ringbuf /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom /home/douwe/.espressif/v6.0/esp-idf/components/esp_security /home/douwe/.espressif/v6.0/esp-idf/components/esp_stdio /home/douwe/.espressif/v6.0/esp-idf/components/esp_system /home/douwe/.espressif/v6.0/esp-idf/components/esp_timer /home/douwe/.espressif/v6.0/esp-idf/components/esp_usb_cdc_rom_console /home/douwe/.espressif/v6.0/esp-idf/components/esptool_py /home/douwe/.espressif/v6.0/esp-idf/components/freertos /home/douwe/.espressif/v6.0/esp-idf/components/hal /home/douwe/.espressif/v6.0/esp-idf/components/heap /home/douwe/.espressif/v6.0/esp-idf/components/log /mnt/douwe/hdd/Projects/SerreklimaatSensor/main /home/douwe/.espressif/v6.0/esp-idf/components/mbedtls /home/douwe/.espressif/v6.0/esp-idf/components/partition_table /home/douwe/.espressif/v6.0/esp-idf/components/pthread /home/douwe/.espressif/v6.0/esp-idf/components/riscv /home/douwe/.espressif/v6.0/esp-idf/components/soc /home/douwe/.espressif/v6.0/esp-idf/components/spi_flash /home/douwe/.espressif/v6.0/esp-idf/components/spiffs /home/douwe/.espressif/v6.0/esp-idf/components/vfs
-- Configuring done (3.8s)
-- Generating done (0.3s)
-- Build files have been written to: /mnt/douwe/hdd/Projects/SerreklimaatSensor/build
[1/10] Building C object esp-idf/main/CMakeFiles/__idf_main.dir/main.c.obj
FAILED: esp-idf/main/CMakeFiles/__idf_main.dir/main.c.obj 
/home/douwe/.espressif/tools/riscv32-esp-elf/esp-15.2.0_20251204/riscv32-esp-elf/bin/riscv32-esp-elf-gcc -DESP_PLATFORM -DIDF_VER=\"v6.0\" -DSOC_MMU_PAGE_SIZE=CONFIG_MMU_PAGE_SIZE -DSOC_XTAL_FREQ_MHZ=CONFIG_XTAL_FREQ -D_GLIBCXX_HAVE_POSIX_SEMAPHORE -D_GLIBCXX_USE_POSIX_SEMAPHORE -D_GNU_SOURCE -D_POSIX_READER_WRITER_LOCKS -I/mnt/douwe/hdd/Projects/SerreklimaatSensor/build/config -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_libc/platform_include -I/home/douwe/.espressif/v6.0/esp-idf/components/freertos/config/include -I/home/douwe/.espressif/v6.0/esp-idf/components/freertos/config/include/freertos -I/home/douwe/.espressif/v6.0/esp-idf/components/freertos/config/riscv/include -I/home/douwe/.espressif/v6.0/esp-idf/components/freertos/FreeRTOS-Kernel/include -I/home/douwe/.espressif/v6.0/esp-idf/components/freertos/FreeRTOS-Kernel/portable/riscv/include -I/home/douwe/.espressif/v6.0/esp-idf/components/freertos/FreeRTOS-Kernel/portable/riscv/include/freertos -I/home/douwe/.espressif/v6.0/esp-idf/components/freertos/esp_additions/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support/include/soc -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support/ldo/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support/debug_probe/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support/etm/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support/mspi_timing_tuning/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support/mspi_timing_tuning/tuning_scheme_impl/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support/power_supply/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support/modem/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support/include/soc/esp32c3 -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support/port/esp32c3/. -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support/port/esp32c3/include -I/home/douwe/.espressif/v6.0/esp-idf/components/heap/include -I/home/douwe/.espressif/v6.0/esp-idf/components/heap/tlsf -I/home/douwe/.espressif/v6.0/esp-idf/components/log/include -I/home/douwe/.espressif/v6.0/esp-idf/components/soc/include -I/home/douwe/.espressif/v6.0/esp-idf/components/soc/esp32c3 -I/home/douwe/.espressif/v6.0/esp-idf/components/soc/esp32c3/include -I/home/douwe/.espressif/v6.0/esp-idf/components/soc/esp32c3/register -I/home/douwe/.espressif/v6.0/esp-idf/components/hal/platform_port/include -I/home/douwe/.espressif/v6.0/esp-idf/components/hal/esp32c3/include -I/home/douwe/.espressif/v6.0/esp-idf/components/hal/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/include/esp32c3 -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3 -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_common/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_system/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_system/port/soc -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_system/port/include/riscv -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_system/port/include/private -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_stdio/include -I/home/douwe/.espressif/v6.0/esp-idf/components/riscv/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_gpio/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_gpio/esp32c3/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_usb/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_usb/esp32c3/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_pmu/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_pmu/esp32c3/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_ana_conv/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_ana_conv/esp32c3/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_dma/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_dma/esp32c3/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_driver_gpio/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_timer/include -I/home/douwe/.espressif/v6.0/esp-idf/components/spi_flash/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_mspi/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_mspi/esp32c3/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_gpspi/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_gpspi/esp32c3/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_clock/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_clock/esp32c3/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_blockdev/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_driver_uart/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_uart/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_uart/esp32c3/include -I/home/douwe/.espressif/v6.0/esp-idf/components/vfs/include -I/home/douwe/.espressif/v6.0/esp-idf/components/spiffs/include -I/home/douwe/.espressif/v6.0/esp-idf/components/esp_partition/include @"/mnt/douwe/hdd/Projects/SerreklimaatSensor/build/toolchain/cflags" -fdiagnostics-color=always -ffunction-sections -fdata-sections -Wall -Werror -Wno-error=unused-function -Wno-error=unused-variable -Wno-error=unused-but-set-variable -Wno-error=deprecated-declarations -Wextra -Wno-error=extra -Wno-unused-parameter -Wno-sign-compare -Wno-enum-conversion -gdwarf-4 -ggdb -Og -fno-shrink-wrap -fmacro-prefix-map=/mnt/douwe/hdd/Projects/SerreklimaatSensor=. -fmacro-prefix-map=/home/douwe/.espressif/v6.0/esp-idf=/IDF -fstrict-volatile-bitfields -fno-jump-tables -fno-tree-switch-conversion -std=gnu23 -Wno-old-style-declaration -fzero-init-padding-bits=all -fno-malloc-dce -MD -MT esp-idf/main/CMakeFiles/__idf_main.dir/main.c.obj -MF esp-idf/main/CMakeFiles/__idf_main.dir/main.c.obj.d -o esp-idf/main/CMakeFiles/__idf_main.dir/main.c.obj -c /mnt/douwe/hdd/Projects/SerreklimaatSensor/main/main.c
/mnt/douwe/hdd/Projects/SerreklimaatSensor/main/main.c: In function 'set_system_time_from_compiler':
/mnt/douwe/hdd/Projects/SerreklimaatSensor/main/main.c:82:5: error: called object 'time' is not a function or function pointer
   82 |     time(&last_known_time); // Save to RTC
      |     ^~~~
/mnt/douwe/hdd/Projects/SerreklimaatSensor/main/main.c:55:10: note: declared here
   55 |     char time[] = __TIME__;
      |          ^~~~
/mnt/douwe/hdd/Projects/SerreklimaatSensor/main/main.c: In function 'led_task':
/mnt/douwe/hdd/Projects/SerreklimaatSensor/main/main.c:148:21: error: 'flickers' undeclared (first use in this function)
  148 |         led_flicker(flickers, fast_flicker);
      |                     ^~~~~~~~
/mnt/douwe/hdd/Projects/SerreklimaatSensor/main/main.c:148:21: note: each undeclared identifier is reported only once for each function it appears in
/mnt/douwe/hdd/Projects/SerreklimaatSensor/main/main.c:148:31: error: 'fast_flicker' undeclared (first use in this function); did you mean 'led_flicker'?
  148 |         led_flicker(flickers, fast_flicker);
      |                               ^~~~~~~~~~~~
      |                               led_flicker
/mnt/douwe/hdd/Projects/SerreklimaatSensor/main/main.c: In function 'measure_task':
/mnt/douwe/hdd/Projects/SerreklimaatSensor/main/main.c:229:9: error: implicit declaration of function 'esp_sleep_enable_ext0_wakeup'; did you mean 'esp_sleep_enable_bt_wakeup'? [-Wimplicit-function-declaration]
  229 |         esp_sleep_enable_ext0_wakeup(BUTTON_PIN, 0);
      |         ^~~~~~~~~~~~~~~~~~~~~~~~~~~~
      |         esp_sleep_enable_bt_wakeup
[2/10] Performing build step for 'bootloader'
[0/1] Re-running CMake...
-- Component directory /home/douwe/.espressif/v6.0/esp-idf/components/mqtt does not contain a CMakeLists.txt file. No component will be added
-- Minimal build - OFF
-- Building ESP-IDF components for target esp32c3
-- ESP-TEE is currently supported only on the esp32c6;esp32h2;esp32c5;esp32c61 SoCs
-- KCONFIG_REPORT_VERBOSITY not set, using default
-- Project sdkconfig file /mnt/douwe/hdd/Projects/SerreklimaatSensor/sdkconfig
Configuration Report                                                            
 ────────────────────────────────────────────────────────────────────────────── 
   Parser Version: 1                                                            
   Verbosity: default                                                           
   Defaults policy: sdkconfig                                                   
   Status: Finished with notifications                                          
                                                                                
  Default Value Mismatch                                                        
   ──────────────────────────────────────────────────────────────────────────   
    Using sdkconfig default values                                              
    Choice symbols with different default selection between sdkconfig and       
    Kconfig                                                                     
    PARTITION_TABLE_TYPE: Kconfig default selection:                            
    PARTITION_TABLE_SINGLE_APP, sdkconfig default selection:                    
    PARTITION_TABLE_CUSTOM                                                      
   ──────────────────────────────────────────────────────────────────────────   
  Multiple Assignments                                                          
   ────────────────────────────────────────────────────                         
    Choice PARTITION_TABLE_TYPE:                                                
        PARTITION_TABLE_SINGLE_APP (default selection)                          
        PARTITION_TABLE_CUSTOM (default selection)                              
        -> using PARTITION_TABLE_CUSTOM                                         
   ────────────────────────────────────────────────────                         
 ────────────────────────────────────────────────────────────────────────────── 
-- Detecting C compiler ABI info
-- Detecting C compiler ABI info - done
-- Detecting CXX compiler ABI info
-- Detecting CXX compiler ABI info - done
-- Detecting C compiler ABI info
-- Detecting C compiler ABI info - done
-- Detecting CXX compiler ABI info
-- Detecting CXX compiler ABI info - done
-- Detecting C compiler ABI info
-- Detecting C compiler ABI info - done
-- Detecting CXX compiler ABI info
-- Detecting CXX compiler ABI info - done
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/riscv/ld/rom.api.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/soc/esp32c3/ld/esp32c3.peripherals.ld
-- Bootloader project name: "bootloader" version: 1
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.api.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.bt_funcs.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.libgcc.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.version.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.libc.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.libc-suboptimal_for_misaligned_mem.ld
-- Components: bootloader bootloader_support efuse esp_app_format esp_blockdev esp_bootloader_format esp_common esp_hal_ana_conv esp_hal_clock esp_hal_dma esp_hal_gpio esp_hal_gpspi esp_hal_mspi esp_hal_pmu esp_hal_rtc_timer esp_hal_security esp_hal_timg esp_hal_uart esp_hal_usb esp_hal_wdt esp_hw_support esp_libc esp_rom esp_security esp_stdio esp_system esptool_py freertos hal log main micro-ecc partition_table riscv soc spi_flash
-- Component paths: /home/douwe/.espressif/v6.0/esp-idf/components/bootloader /home/douwe/.espressif/v6.0/esp-idf/components/bootloader_support /home/douwe/.espressif/v6.0/esp-idf/components/efuse /home/douwe/.espressif/v6.0/esp-idf/components/esp_app_format /home/douwe/.espressif/v6.0/esp-idf/components/esp_blockdev /home/douwe/.espressif/v6.0/esp-idf/components/esp_bootloader_format /home/douwe/.espressif/v6.0/esp-idf/components/esp_common /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_ana_conv /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_clock /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_dma /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_gpio /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_gpspi /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_mspi /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_pmu /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_rtc_timer /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_security /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_timg /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_uart /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_usb /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_wdt /home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support /home/douwe/.espressif/v6.0/esp-idf/components/esp_libc /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom /home/douwe/.espressif/v6.0/esp-idf/components/esp_security /home/douwe/.espressif/v6.0/esp-idf/components/esp_stdio /home/douwe/.espressif/v6.0/esp-idf/components/esp_system /home/douwe/.espressif/v6.0/esp-idf/components/esptool_py /home/douwe/.espressif/v6.0/esp-idf/components/freertos /home/douwe/.espressif/v6.0/esp-idf/components/hal /home/douwe/.espressif/v6.0/esp-idf/components/log /home/douwe/.espressif/v6.0/esp-idf/components/bootloader/subproject/main /home/douwe/.espressif/v6.0/esp-idf/components/bootloader/subproject/components/micro-ecc /home/douwe/.espressif/v6.0/esp-idf/components/partition_table /home/douwe/.espressif/v6.0/esp-idf/components/riscv /home/douwe/.espressif/v6.0/esp-idf/components/soc /home/douwe/.espressif/v6.0/esp-idf/components/spi_flash
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/bootloader/subproject/main/ld/esp32c3/bootloader.ld.in
--   -> Preprocessing .in script: /home/douwe/.espressif/v6.0/esp-idf/components/bootloader/subproject/main/ld/esp32c3/bootloader.ld.in
-- Configuring done (2.3s)
-- Generating done (0.1s)
-- Build files have been written to: /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/bootloader
[1/2] cd /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/bootloader && /home/douwe/.espressif/tools/python/v6.0/venv/bin/python /home/douwe/.espressif/v6.0/esp-idf/components/partition_table/check_sizes.py --offset 0x8000 bootloader 0x0 /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/bootloader/bootloader.bin
Bootloader binary size 0x5250 bytes. 0x2db0 bytes (36%) free.
ninja: build stopped: subcommand failed.
