Command: /home/douwe/.espressif/tools/python/v6.0/venv/bin/python /home/douwe/.espressif/v6.0/esp-idf/tools/idf_monitor.py -p /dev/ttyACM0 -b 115200 --toolchain-prefix riscv32-esp-elf- --target esp32c3 --revision 3 --decode-panic backtrace /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/dht11_reader.elf /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/bootloader/bootloader.elf -m '/home/douwe/.espressif/tools/python/v6.0/venv/bin/python' '/home/douwe/.espressif/v6.0/esp-idf/tools/idf.py'
[0;33m--- esp-idf-monitor 1.9.0 on /dev/ttyACM0 115200[0m
[0;33m--- Quit: Ctrl+] | Menu: Ctrl+T | Help: Ctrl+T followed by Ctrl+H[0m
[0m--- 0x4004c51e: [0;33muart_rx_one_char[0m[0m in [0;32mROM[0m
[1;31m--- Error: device reports readiness to read but returned no data (device disconnected or multiple access on port?)[0m
[0;33m--- Waiting for the device to reconnect[0m[0;33m.[0m[0;33m[0m
[1;31m--- Error: device reports readiness to read but returned no data (device disconnected or multiple access on port?)[0m
[0;33m--- Waiting for the device to reconnect[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m[0m
[1;31m--- Error: device reports readiness to read but returned no data (device disconnected or multiple access on port?)[0m
[0;33m--- Waiting for the device to reconnect[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m.[0m[0;33m[0m
[0m
