Command: ninja all
[0/1] Re-running CMake...
-- Component directory /home/douwe/.espressif/v6.0/esp-idf/components/mqtt does not contain a CMakeLists.txt file. No component will be added
-- Minimal build - ON
-- Building ESP-IDF components for target esp32c3
-- ESP-TEE is currently supported only on the esp32c6;esp32h2;esp32c5;esp32c61 SoCs
-- KCONFIG_REPORT_VERBOSITY not set, using default
-- Project sdkconfig file /mnt/douwe/hdd/Projects/SerreklimaatSensor/sdkconfig
-- Detecting C compiler ABI info
-- Detecting C compiler ABI info - done
-- Detecting CXX compiler ABI info
-- Detecting CXX compiler ABI info - done
-- Detecting C compiler ABI info
-- Detecting C compiler ABI info - done
-- Detecting CXX compiler ABI info
-- Detecting CXX compiler ABI info - done
-- Detecting C compiler ABI info
-- Detecting C compiler ABI info - done
-- Detecting CXX compiler ABI info
-- Detecting CXX compiler ABI info - done
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/riscv/ld/rom.api.ld
-- App "dht11_reader" version: 1d246d6-dirty
-- Setting up mbedtls configuration
-- Linkage type is PUBLIC
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_system/ld/esp32c3/memory.ld.in
--   -> Preprocessing .in script: /home/douwe/.espressif/v6.0/esp-idf/components/esp_system/ld/esp32c3/memory.ld.in
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_system/ld/esp32c3/sections.ld.in
--   -> Preprocessing .in script: /home/douwe/.espressif/v6.0/esp-idf/components/esp_system/ld/esp32c3/sections.ld.in
--   -> Applying ldgen processing: /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/esp-idf/esp_system/ld/sections.ld.in
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.api.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.bt_funcs.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.libgcc.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.version.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ble_master.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ble_50.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ble_smp.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ble_dtm.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ble_test.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.ble_scan.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.eco3.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.eco3_bt_funcs.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom/esp32c3/ld/esp32c3.rom.libc.ld
-- Adding linker script /home/douwe/.espressif/v6.0/esp-idf/components/soc/esp32c3/ld/esp32c3.peripherals.ld
-- Components: app_update bootloader bootloader_support cxx efuse esp_app_format esp_blockdev esp_bootloader_format esp_common esp_driver_dma esp_driver_gpio esp_driver_uart esp_driver_usb_serial_jtag esp_hal_ana_conv esp_hal_clock esp_hal_dma esp_hal_gpio esp_hal_gpspi esp_hal_i2s esp_hal_mspi esp_hal_pmu esp_hal_rtc_timer esp_hal_security esp_hal_timg esp_hal_touch_sens esp_hal_uart esp_hal_usb esp_hal_wdt esp_hw_support esp_libc esp_mm esp_partition esp_pm esp_psram esp_ringbuf esp_rom esp_security esp_stdio esp_system esp_timer esp_usb_cdc_rom_console esptool_py freertos hal heap log main mbedtls partition_table pthread riscv soc spi_flash spiffs vfs
-- Component paths: /home/douwe/.espressif/v6.0/esp-idf/components/app_update /home/douwe/.espressif/v6.0/esp-idf/components/bootloader /home/douwe/.espressif/v6.0/esp-idf/components/bootloader_support /home/douwe/.espressif/v6.0/esp-idf/components/cxx /home/douwe/.espressif/v6.0/esp-idf/components/efuse /home/douwe/.espressif/v6.0/esp-idf/components/esp_app_format /home/douwe/.espressif/v6.0/esp-idf/components/esp_blockdev /home/douwe/.espressif/v6.0/esp-idf/components/esp_bootloader_format /home/douwe/.espressif/v6.0/esp-idf/components/esp_common /home/douwe/.espressif/v6.0/esp-idf/components/esp_driver_dma /home/douwe/.espressif/v6.0/esp-idf/components/esp_driver_gpio /home/douwe/.espressif/v6.0/esp-idf/components/esp_driver_uart /home/douwe/.espressif/v6.0/esp-idf/components/esp_driver_usb_serial_jtag /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_ana_conv /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_clock /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_dma /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_gpio /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_gpspi /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_i2s /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_mspi /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_pmu /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_rtc_timer /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_security /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_timg /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_touch_sens /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_uart /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_usb /home/douwe/.espressif/v6.0/esp-idf/components/esp_hal_wdt /home/douwe/.espressif/v6.0/esp-idf/components/esp_hw_support /home/douwe/.espressif/v6.0/esp-idf/components/esp_libc /home/douwe/.espressif/v6.0/esp-idf/components/esp_mm /home/douwe/.espressif/v6.0/esp-idf/components/esp_partition /home/douwe/.espressif/v6.0/esp-idf/components/esp_pm /home/douwe/.espressif/v6.0/esp-idf/components/esp_psram /home/douwe/.espressif/v6.0/esp-idf/components/esp_ringbuf /home/douwe/.espressif/v6.0/esp-idf/components/esp_rom /home/douwe/.espressif/v6.0/esp-idf/components/esp_security /home/douwe/.espressif/v6.0/esp-idf/components/esp_stdio /home/douwe/.espressif/v6.0/esp-idf/components/esp_system /home/douwe/.espressif/v6.0/esp-idf/components/esp_timer /home/douwe/.espressif/v6.0/esp-idf/components/esp_usb_cdc_rom_console /home/douwe/.espressif/v6.0/esp-idf/components/esptool_py /home/douwe/.espressif/v6.0/esp-idf/components/freertos /home/douwe/.espressif/v6.0/esp-idf/components/hal /home/douwe/.espressif/v6.0/esp-idf/components/heap /home/douwe/.espressif/v6.0/esp-idf/components/log /mnt/douwe/hdd/Projects/SerreklimaatSensor/main /home/douwe/.espressif/v6.0/esp-idf/components/mbedtls /home/douwe/.espressif/v6.0/esp-idf/components/partition_table /home/douwe/.espressif/v6.0/esp-idf/components/pthread /home/douwe/.espressif/v6.0/esp-idf/components/riscv /home/douwe/.espressif/v6.0/esp-idf/components/soc /home/douwe/.espressif/v6.0/esp-idf/components/spi_flash /home/douwe/.espressif/v6.0/esp-idf/components/spiffs /home/douwe/.espressif/v6.0/esp-idf/components/vfs
-- Configuring done (3.8s)
-- Generating done (0.3s)
-- Build files have been written to: /mnt/douwe/hdd/Projects/SerreklimaatSensor/build
[1/10] Performing build step for 'bootloader'
[1/1] cd /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/bootloader && /home/douwe/.espressif/tools/python/v6.0/venv/bin/python /home/douwe/.espressif/v6.0/esp-idf/components/partition_table/check_sizes.py --offset 0x8000 bootloader 0x0 /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/bootloader/bootloader.bin
Bootloader binary size 0x5250 bytes. 0x2db0 bytes (36%) free.
[2/10] No install step for 'bootloader'
[3/10] Completed 'bootloader'
[4/10] Building C object esp-idf/main/CMakeFiles/__idf_main.dir/main.c.obj
[5/10] Linking C static library esp-idf/main/libmain.a
[6/10] Generating esp-idf/esp_system/ld/sections.ld
[7/10] Linking CXX executable dht11_reader.elf
[8/10] Generating binary image from built executable
esptool v5.3.dev2
Creating ESP32-C3 image...
Merged 2 ELF sections.
Successfully created ESP32-C3 image.
Generated /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/dht11_reader.bin
[9/10] cd /mnt/douwe/hdd/Projects/SerreklimaatSensor/build && /home/douwe/.espressif/tools/python/v6.0/venv/bin/python /home/douwe/.espressif/v6.0/esp-idf/components/partition_table/check_sizes.py --offset 0x8000 partition --type app /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/partition_table/partition-table.bin /mnt/douwe/hdd/Projects/SerreklimaatSensor/build/dht11_reader.bin
dht11_reader.bin binary size 0x2cdd0 bytes. Smallest app partition is 0x1e0000 bytes. 0x1b3230 bytes (91%) free.
